# Copyright (c) 2014-present PlatformIO <contact@platformio.org>
#
# Licensed under the Apache License, Version 2.0 (the "License");
# you may not use this file except in compliance with the License.
# You may obtain a copy of the License at
#
#    http://www.apache.org/licenses/LICENSE-2.0
#
# Unless required by applicable law or agreed to in writing, software
# distributed under the License is distributed on an "AS IS" BASIS,
# WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
# See the License for the specific language governing permissions and
# limitations under the License.

#####################################################################################
#
# INSTALLATION
#
# Please visit > https://docs.platformio.org/en/latest/core/installation/udev-rules.html
#
#####################################################################################

#
# Boards
#

# CP210X USB UART
ATTRS{idVendor}=="10c4", ATTRS{idProduct}=="ea[67][013]", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"
ATTRS{idVendor}=="10c4", ATTRS{idProduct}=="80a9", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# FT231XS USB UART
ATTRS{idVendor}=="0403", ATTRS{idProduct}=="6015", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Prolific Technology, Inc. PL2303 Serial Port
ATTRS{idVendor}=="067b", ATTRS{idProduct}=="2303", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# QinHeng Electronics HL-340 USB-Serial adapter
ATTRS{idVendor}=="1a86", ATTRS{idProduct}=="7523", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"
# QinHeng Electronics CH343 USB-Serial adapter
ATTRS{idVendor}=="1a86", ATTRS{idProduct}=="55d3", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"
# QinHeng Electronics CH9102 USB-Serial adapter
ATTRS{idVendor}=="1a86", ATTRS{idProduct}=="55d4", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Arduino boards
ATTRS{idVendor}=="2341", ATTRS{idProduct}=="[08][023]*", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"
ATTRS{idVendor}=="2a03", ATTRS{idProduct}=="[08][02]*", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Arduino SAM-BA
ATTRS{idVendor}=="03eb", ATTRS{idProduct}=="6124", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{MTP_NO_PROBE}="1"

# Digistump boards
ATTRS{idVendor}=="16d0", ATTRS{idProduct}=="0753", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Maple with DFU
ATTRS{idVendor}=="1eaf", ATTRS{idProduct}=="000[34]", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# USBtiny
ATTRS{idProduct}=="0c9f", ATTRS{idVendor}=="1781", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# USBasp V2.0
ATTRS{idVendor}=="16c0", ATTRS{idProduct}=="05dc", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Teensy boards
ATTRS{idVendor}=="16c0", ATTRS{idProduct}=="04[789B]?", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"
ATTRS{idVendor}=="16c0", ATTRS{idProduct}=="04[789A]?", ENV{MTP_NO_PROBE}="1"
SUBSYSTEMS=="usb", ATTRS{idVendor}=="16c0", ATTRS{idProduct}=="04[789ABCD]?", MODE:="0666"
KERNEL=="ttyACM*", ATTRS{idVendor}=="16c0", ATTRS{idProduct}=="04[789B]?", MODE:="0666"

# TI Stellaris Launchpad
ATTRS{idVendor}=="1cbe", ATTRS{idProduct}=="00fd", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# TI MSP430 Launchpad
ATTRS{idVendor}=="0451", ATTRS{idProduct}=="f432", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# GD32V DFU Bootloader
ATTRS{idVendor}=="28e9", ATTRS{idProduct}=="0189", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# FireBeetle-ESP32
ATTRS{idVendor}=="1a86", ATTRS{idProduct}=="7522", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Wio Terminal
ATTRS{idVendor}=="2886", ATTRS{idProduct}=="[08]02d", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Raspberry Pi Pico
ATTRS{idVendor}=="2e8a", ATTRS{idProduct}=="[01]*", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# AIR32F103
ATTRS{idVendor}=="0d28", ATTRS{idProduct}=="0204", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# STM32 virtual COM port
ATTRS{idVendor}=="0483", ATTRS{idProduct}=="5740", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

#
# Debuggers
#

# Black Magic Probe
SUBSYSTEM=="tty", ATTRS{interface}=="Black Magic GDB Server", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"
SUBSYSTEM=="tty", ATTRS{interface}=="Black Magic UART Port", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# opendous and estick
ATTRS{idVendor}=="03eb", ATTRS{idProduct}=="204f", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Original FT232/FT245/FT2232/FT232H/FT4232
ATTRS{idVendor}=="0403", ATTRS{idProduct}=="60[01][104]", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# DISTORTEC JTAG-lock-pick Tiny 2
ATTRS{idVendor}=="0403", ATTRS{idProduct}=="8220", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# TUMPA, TUMPA Lite
ATTRS{idVendor}=="0403", ATTRS{idProduct}=="8a9[89]", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# XDS100v2
ATTRS{idVendor}=="0403", ATTRS{idProduct}=="a6d0", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Xverve Signalyzer Tool (DT-USB-ST), Signalyzer LITE (DT-USB-SLITE)
ATTRS{idVendor}=="0403", ATTRS{idProduct}=="bca[01]", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# TI/Luminary Stellaris Evaluation Board FTDI (several)
ATTRS{idVendor}=="0403", ATTRS{idProduct}=="bcd[9a]", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# egnite Turtelizer 2
ATTRS{idVendor}=="0403", ATTRS{idProduct}=="bdc8", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Section5 ICEbear
ATTRS{idVendor}=="0403", ATTRS{idProduct}=="c14[01]", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Amontec JTAGkey and JTAGkey-tiny
ATTRS{idVendor}=="0403", ATTRS{idProduct}=="cff8", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# TI ICDI
ATTRS{idVendor}=="0451", ATTRS{idProduct}=="c32a", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# STLink probes
ATTRS{idVendor}=="0483", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Hilscher NXHX Boards
ATTRS{idVendor}=="0640", ATTRS{idProduct}=="0028", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Hitex probes
ATTRS{idVendor}=="0640", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Altera USB Blaster
ATTRS{idVendor}=="09fb", ATTRS{idProduct}=="6001", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Amontec JTAGkey-HiSpeed
ATTRS{idVendor}=="0fbb", ATTRS{idProduct}=="1000", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# SEGGER J-Link
ATTRS{idVendor}=="1366", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Raisonance RLink
ATTRS{idVendor}=="138e", ATTRS{idProduct}=="9000", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Debug Board for Neo1973
ATTRS{idVendor}=="1457", ATTRS{idProduct}=="5118", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Olimex probes
ATTRS{idVendor}=="15ba", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# USBprog with OpenOCD firmware
ATTRS{idVendor}=="1781", ATTRS{idProduct}=="0c63", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# TI/Luminary Stellaris In-Circuit Debug Interface (ICDI) Board
ATTRS{idVendor}=="1cbe", ATTRS{idProduct}=="00fd", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Marvell Sheevaplug
ATTRS{idVendor}=="9e88", ATTRS{idProduct}=="9e8f", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Keil Software, Inc. ULink
ATTRS{idVendor}=="c251", ATTRS{idProduct}=="2710", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# CMSIS-DAP compatible adapters
ATTRS{product}=="*CMSIS-DAP*", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Atmel AVR Dragon
ATTRS{idVendor}=="03eb", ATTRS{idProduct}=="2107", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Espressif USB JTAG/serial debug unit
ATTRS{idVendor}=="303a", ATTRS{idProduct}=="1001", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"

# Zephyr framework USB CDC-ACM
ATTRS{idVendor}=="2fe3", ATTRS{idProduct}=="0100", MODE="0666", ENV{ID_MM_DEVICE_IGNORE}="1", ENV{ID_MM_PORT_IGNORE}="1"